**Power Extension Cable**

**PDS-CAB-PWCEXT-14**

|  |
| --- |
| **Feature** |
| Wire End Rating | NEMA TYPE 3, 4 |
| Wire End Hazardous Area Rating | Class I, Divisions 1 & 2, Groups B, C, DClass I, Zones 1 & 2, Groups IIB + H², IIAClass II, Divisions 1 & 2, Groups F, GClass III |
| Wire End Connection Rating | 15 Amp 125VAC |
| Length | 100 ft / 30.48 m300ft / 91.44 m |
| Cable Type | 14 AWG-3C Portable Cord SOOW 600V -40C to +90C, CPE JktUL, CSA, MSHA |
|  |  |
| **Product Variants** |  |
| PDS-CAB-PWCEXT-14-100 – Power extension cable, 100-foot |
| PDS-CAB-PWCEXT-14-300 – Power extension cable, 300-foot |
|  |
| **Related Products** |
| XPL-R5 – Explosion-Proof Light |
|  |
|  |
|  |



The cable certified for portable use in hazardous locations where flammable gases, liquids, vapors, combustible dusts, or fibers are present; this durable cable provides extended power to your needs reliably in wet, corrosive, and hazardous areas, both indoors and outdoors.